Sveasoft firmware for the WRT54G V1.0, 1.1. and 2.0 and WRT54GS 1.0

Version Alchemy-pre5.1

USE OF THIS FIRMWARE IS AT YOUR OWN RISK!!

This firmware is distributed under the GPL license. The firmware can
be re-distributed in source and binary forms. If you choose to re-distribute
this firmware in binary form you MUST make the source code available. You
are also responsible for any support issues for those people to whom you
distribute the firmware.

This firmware is pre-release firmware distributed by Sveasoft directly to
Sveasoft subscribers. Subscribers are entitled to Sveasoft support and,
should they choose to, may re-distribute this firmware under the GPL license.
Re-distribution terminates Sveasoft subscribers rights though it does not
terminate any rights conferred to subscribers or any other parties under
the GPL license.

Alchemy-pre5.1 is a unified firmware for both G and GS models. This firmware
can only be upgraded using the web interface. IF YOU HAVE A FIRMWARE UPGRADE
FAILURE WITH ALCHEMY - you must use an older firmware version whose size is
under 3,145,000 bytes and reflash using tftp. Reflashing with tftp will not
work with firmware versions larger than 3,145,000 bytes in size.

Alchemy-pre5.1 firmware fixes from pre5.0
	QoS web fixes
	QoS internal fixes
	NAS fixes

Alchemy firmware additions from Satori-pre3.11:

	Multi-level QoS (see web interface)
	Ebtables 2.03
	Iptables 1.2.11
	Multiple client fix for client mode
	Optimization of kernel QoS code
	Busybox1.0-pre10
	Dropbear SSH 0.42
	802.11x/WPA support on WDS interfaces
	Zebra OSPF with WDS interface support
	Squashfs V2.0 file system
	
All of these new features should be considered experimental. Always reset your router
to defaults after upgrading.
