Alchemy-pre5.4a is a unified firmware for both G and GS models. This firmware
can only be upgraded using the web interface. IF YOU HAVE A FIRMWARE UPGRADE
FAILURE WITH ALCHEMY - you must use an older firmware version whose size is
under 3,145,000 bytes and reflash using tftp. Reflashing with tftp will not
work with firmware versions larger than 3,145,000 bytes in size.

All of these new features should be considered experimental. 
Always reset your router to defaults after upgrading

Alchemy-pre5.4a additions from Alchemy-pre5.4

Fixed critical bug with bridging code

Alchemy-pre5.4 additions from Alchemy-pre5.3

Dropbear V0.44test4 including ssh client
Bugfixes for site survey in Status->Wireless
Bugfixes Backup & Restore
Bugfixes to saving parameters via SSL
Bugfixes to UPnP, PPTP, and L2TP
Bugfixes to DHCP
Added OSPF route balancing and web interface when expert_mode=1
Added alternate DNS servers
- used by dnsmasq if DHCP is not active. 
- need to set altdns1, altdns2, altdns3 nvram parameter
Many many small bugfixes and tweaks

Alchemy-pre5.3 additions from Alchemy-pre5.2.3

Dropbear V0.44test3 including ssh client
Busybox V1.0-RC3
Linksys source code and drivers V2.04.4
Bugfixes for site survey in Status->Wireless
Bugfixes Backup & Restore
Chillispot 0.96
Fixed WPA for WDS
Added ipp2p filter for P2P blocking and QoS
Fixed Access Restrictions bug
Many many small bugfixes and tweaks

Special thanks to: 

Traveller for WPA testing and feedback
Wolf for extensive fixes, features, testing, and support
Lonewolf for OSPF additions, testing, and feedback 
Reformed for a complete review and bugfixing of Linksys PPT, L2TP, UPnP, and DHCP code

