Firmware_Alchemy-pre5.2.2
     
SVEASOFT FIRMWARE FOR THE LINKSYS WRT54G AND WRT54GS ROUTER. USE IS AT YOUR OWN RISK.

This firmware is for WRT54G V1.0, V1.1, V2.0 and WRT54GS routers only.

This file is distributed to Sveasoft subscribers only. Redistribution is allowed under 
the GPL license. However, redistribution terminates Sveasoft subscription rights.

Alchemy-pre5.2.2 is a unified firmware for both G and GS models. This firmware
can only be upgraded using the web interface. IF YOU HAVE A FIRMWARE UPGRADE
FAILURE WITH ALCHEMY - you must use an older firmware version whose size is
under 3,145,000 bytes and reflash using tftp. Reflashing with tftp will not
work with firmware versions larger than 3,145,000 bytes in size.

Alchemy-pre5.2.2 addtions from Alchemy-pre5.2.1

This is a bug fix release

fixes to client mode and WEP
fixes for save on V1.0, V1.1 models
QoS ingress policing fixes
firewall fixes
development code cleanup


Alchemy-pre5.2.1 addtions from Alchemy-pre5.2

Firewall and PPPoE bug fixes


Alchemy-pre5.2 additons from Alchemy-pre5.1

QoS ingress policing with IMQ
- means QoS is active both for incoming and outgoing data
Port Triggering
Hotspot support (chillispot included, needs manual setup)
Client mode runs wireless device as the WAN device
Multiple attached device support for client mode
PPTP Internet connection can be encrypted/unencrypted
PPTP client upgrade to V1.5
L2TP support
Wireless MAC clone support
OSPF improvements
SNMP Support
WOL Support
Ntop remote statistics support (must be invoked manually)
Packet8 QoS Support
Add/Edit Services fixes
VLAN support in web interface
Access restriction fixes for L7 services
Fix for disabled firewall security issues
Fix for crond bugs
Latest Busybox version upgrade
PPTP server fixes and improvements

All of these new features should be considered experimental. Always reset 
your router to defaults after upgrading.
