IMPORTANT NOTE: 
This is my second tag-free release. Sveasoft increased the amount of tagged files and added a new thing which I hadn't seen before: a hidden .reg file.
I have set it to zero and I hope everything works fine without it. All other tagged files (gif,asp) have been cleaned and should not contain any tags.
This mean however that I had to rebuild the entire filesystem.
So PLEASE be careful with this release, it should work fine but as always I can't offer any guarantees.

RELEASE INFO:
This is a fork from the Alchemy-6.0rc1 CVS made by Wolf.
It is probably the last Alchemy based firmware that has IPv6 which is why I am releasing it.
There will very soon be a public release of Alchemy, in the meantime this should be a very good, stable version to work with.
I included the CHANGELOG so you can see what's new.
I can not offer source code for this yet because neither Sveasoft nor Wolf have made it available.
So it's their GPL violation, not mine.

Have fun with the firmware and big thanks to two good friends for the supply :)
TheIndividual

For news and links to my mirrors, visit my slashdot journal http://slashdot.org/~TheIndividual/journal/
Post comments, questions or anything else at http://forum.bsr-clan.de/viewforum.php?f=12


## Official comments by Wolf@sveasoft starts here ##
This is my final Alchemy-based release 

The following are feature differences between this release and the mainline version it is based on: 
* Basic Chillispot web interface 
* Full IPv6 (layer 2-3) support via CLI (nvram: ipv6_enable) 
* radvd for IPv6 address assignment via CLI (nvram: radvd_enable & radvd_conf) 
* Web interface option for bridged or routed client mode 
* Option on the Admin->Log page for adjusting logging level *NEW* 

Bridged client mode broadcasts forwarding and DHCP relay will not work with this release. DHCP relay will be worked on for my Talisman builds. 

Please do speed tests for this release aswell. See the speed test request post above about the method I wish to be used.


For IPv6 support, set ipv6_enable to "1" and commit/reboot. Use the "ip" command to configure. 

For radvd, set radvd_enable to "1" and put an radvd configuration in radvd_conf ... then reboot. This will create /tmp/radvd.conf and load radvd with that configuration. 

For more information about configuring IPv6 and radvd, google :)